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Panasonic KX-TD1232 Programming Codes
Press PROGRAM STAR POUND 1234 at main phone or managers phone to enter programming mode
Code Description (Default)
000 Time/Date Setting
001 System Speed Dial (00 to 99 on older software versions) (000 to 499 on newer software versions)
002 System Speed Dial Name Set (10 Characters maximum)
003 Extension Number Assignment (01=101 etc.)
004 Extension Name Set
005 Flexible CO Button Assignment
0= Single CO 1= DSS Key 2= One Touch Dialing Key
3= MWL 4= FWD/DND 5= Save
6= Account 70= Conference 71= Log In/Log Out
72= Phantom 73= Night 8= Voice Mail Transfer
90= Two-Way Record 91= Two-Way Transfe 92= Live Call Screening
93= Live Call * = Loop CO # = Group CO
 Screening Cancel
CO Key=Ringer Frequency
006 Operator/Manager Extension Assignment
007 DSS Console Port and Paired Telephone Assignment
008 Absent Messages
009 Quick Dial Number Set
012 ISDN Extension Number Set
013 ISDN Extension Name Set
014 Voice Mail Name Set
SYSTEM Programming
100 Flexible Numbering
101 Day/Night Switching Mode (Manual/Auto)
102 Day/Night Starting Time
103 Automatic Access Outside Line Assignment Sequence
104 Account codes
106 Station Hunting Type
107 System Password
108 Automatic Hold by CO/DSS Button
109 Expansion Unit Type
110 Caller ID Code set
111 Caller ID Name Set
112 Network Type Assignment
113 Voice Mail Status DTMF Set
114 Voice mail Command DTMF Set
115 Adjust time
116 ROM Version Display
117 Voice Mail Number
118 Voice Mail Extension Number Assignment
119 Voice Mail Extension Group Assignment
120 User Password
121 Walking COS Password
122 UCD Overflow
123 UCD Time Table
124 Phantom Extension Number Assignment
125 Area Code Assignment
126 Caller ID Modification for Local Call
127 Caller ID Modification for Long Distance Call
128 PBX Code
130 Message Waiting Control
131 Message Waiting Lamp Assignment
132 Message Waiting Port Assignment
133 Caller ID Extension Assignment
134 Hotel Application
135 DID Number Conversion Selection
136 DID Number Assignment
137 DID Extension Day
138 DID Extension Night
139 DID Extension Name Set
148 Off Hook Monitor
150 Lunch Service Starting/Ending time
151 Break Service Starting/Ending time
TIMER Programming
200 Hold Recall Time
201 Transfer Recall Time
202 Call Forwarding-No Answer Time
203 Intercept Time
204 Pickup Dial Waiting Time
205 Extension-To-Outside Line Call Duration time
206 Outside-To-Outside Line Call Duration time
207 First Digit Time
208 Inter Digit Time
211 Dial Start Time
212 Call Duration Count Start Time
213 DISA Delayed Answer Time
214 DISA Prolong time
215 DISA Outgoing Message Time
216 Message Waiting Ring Interval Time
217 Timed Reminder Alarm Ring Time
218 DISA AA Wait Time
219 Call Park Recall Time
220 TIE First/Inter Digit 
TRS/ARS Programming
300 TRS Override for System Speed Dialing
301 TRS Denied Code Entry restricts Level 2 through 6
302 TRS Denied Code Entry restricts Level 3 through 6
303 TRS Denied Code Entry restricts Level 4 through 6
304 TRS Denied Code Entry restricts Level 5 through 6
305 TRS Denied Code Entry restricts Level 6
306 Applies to level 2
307 Applies to level 2 through 3
308 Applies to level 2 through 4
309 Applies to level 2 through 5
310 Applies to level 2 through 6
311 Special Carries Access Codes
312 ARS Mode
313 ARS Time
314 ARS Leading Digit Entry for Plan 1
315 ARS Leading Digit Entry for Plan 2
316 ARS Leading Digit Entry for Plan 3
317 ARS Leading Digit Entry for Plan 4
318 ARS Leading Digit Entry for Plan 5
319 ARS Leading Digit Entry for Plan 6
320 ARS Leading Digit Entry for Plan 7
321 ARS Leading Digit Entry for Plan 8
322 ARS Routing Plan 1
323 ARS Routing Plan 2
324 ARS Routing Plan 3
325 ARS Routing Plan 4
326 ARS Routing Plan 5
327 ARS Routing Plan 6
328 ARS Routing Plan 7
329 ARS Routing Plan 8
330 ARS Modify Removed Digit
331 ARS Modify Added Number
332 Extra Entry Table Selection
333 TRS Entry Code Assignment for Extra Table
334 Emergency Dial Number set
340 TIE Line Routing Table
341 TIE Modify Removed/Added digit
OUTSIDE LINE ASSIGNMENT Assignment Programming
400 Outside Line Connection Assignment 
401 Outside Line Group Assignment
402 Dial Mode Selection
403 Pulse Speed Selection
404 DTMF Time
405 CPC Signal Detection Incoming 
406 Caller ID Assignment
407 DIL 1:1 Extension Day (Assign DAY Ringing by Port to ONE Station Only)
408 DIL 1:1 Extension NIGHT (Assign NIGHT Ringing by Port to ONE Station Only)
409 Intercept Extension-Day 
410 Intercept Extension-Night 
411 Host PBX Access Codes
412 Pause Time
413 Flash Time
414 Disconnect Time
415 CPC Signal Detection Outgoing Set
416 Reverse Circuit Assignment
417 Outside Line Name Assignment
419 ISDN Outgoing CLIR Service Assignment
420 ISDN Ring Service Assignment
423 ISDN Port Type
424 ISDN Layer 1 Active Mode
425 ISDN Configuration
426 ISDN Data Link mode
427 ISDN TEI Mode
428 ISDN Extension Multiple Directory Number
429 ISDN Extension Progress tone
430 DID/TIE Format Number Assignment
431 DID/TIE Incoming Assignment
432 DID/TIE Outgoing Assignment
433 DID/TIE Subscriber Number Removed Digit
434 DID/TIE Added Number
435 DID/TIE Wink time Out Assignment
436 CO-to-TIE Transfer
437 TIE-to-CO Transfer
438 TIE-to-TIE Transfer
439 TIE Security Type
440 Line Hunting Sequence
453 SPID Assignment
454 DN Assignment
455 Extension Ringing Assignment-Day for ISDN
456 Extension Ringing Assignment-Night for ISDN
457 DIL 1:1 Lunch Group
458 DIL 1:1 Break Group
COS Programming
500 Toll Restriction Level-Day
501 Toll Restriction Level-Night
502 Extension-to-Outside Line Call Duration Limit
503 Call Transfer to Outside Line
504 Call Forward to Outside Line
505 Executive Busy Override
506 Executive Busy Override 
507 Do Not Disturb Override
508 Account Code Entry Mode
509 Off-Hook Call Announcement (OHCA)
510 Night Service Access
511 PITS Programming Level
EXTENSION Programming
600 Extra Device Port
601 Class of Service
602 Extension Group Assignment
603 DIL 1:N Extension and Delayed Ringing-Day (For any phone) 
604 DIL 1:N Extension and Delayed Ringing-Night (For any phone) 
605 Outgoing Line Access-Day 
606 Outgoing Line Access-Night 
607 Doorphone Ringing Assignment-DAY
608 Doorphone Ringing Assignment-NIGHT
609 Voice Mail Access Codes
610 Live Call Screening Recording Mode Asssignment
613 ISDN Calss of Service
614 Outgoing Line Assignment DAY (For ISDN Extension)
615 Outgoing Line Assignment NIGHT (For ISDN Extension)
619 Extension Call Forwarding-No Answer Time
620 Lunch/Break Group Assignment
621 Cordless PITS Extension Port
T1 Programming
700 All T1 programming codes are in the 700's. Believe me, you need a laptop for this.
Resource Programming
800 SMDR Incoming/Outgoing Call Log Printout (Default: Outgoing: ALL Incoming: ON)
801 SMDR Format (Page Length 66 Skip Perforation 0)
802 System Data Printout
803 Music Source Use (DEFAULT: HOLD and BGM is set to Music One)
804 External Pager BGM (Default: DISABLE)
805 External Pager Confirmation Tone (Default: ON)
806 Serial Interface (RS-232C) Parameters (CR+LF, Baud Rate 9600, Word Length 8, Parity: MARK, Stop 
Bit: 1)
809 DISA Security Type
809 DISA Tone Detection
811 DISA User Codes812 DISA DTMF Repeat
813 Floating Number Assignment
814 Modem Standard (Default: BELL)
815 DISA Built-in Auto Attendant (Default: DISABLE)
817 KX-TD 197 and KX-TD 198 Baud Rate Set (Default V.34-9600)
OPTIONAL PROGRAMMING: Only most changed features are listed
900
Area 01 1 Sound Source During Transfer 0: Ringback Tone 1: Music On Hold
Area 01 3 Result of FLASH on proprietary telephones 0: Disconnect 1: External Feature Access such
as Centrex or TELCO Call Waiting
Area 01 9 Result of pressing the hookswitch lightly 0: Consultation Hold 1: Disconnect
(SLT Only)
Area 02 3 Allows you to remove confirmation tone 0: Disable 1: Enable
4. By default, a beep tone sounds when
a 3-party conference is started or ended
Area 02 6 Allows you to remove Confirmation 0: Extension Number 1: Free
Tone 3. This tone is sent when a conversation
is established just after dialing the feature
number for accessing the following: Call
Pickup, Paging, Paging Answer, TAFAS,
Hold Retrieve and Call Park Retrieve.
Area 05 1 Enables or Disables the automatic time 0: Enable 1: Disable
adjustment By caller ID information once
a day by the first call received after 3:00 AM
Area 09 4,3 Assigns the display of FWD/DND on LED. 11: MWL Flash /DND On
Reset system after setting this assignment 10: MWL On/DND On
01: MWL On/DND Flash
00: MWL Flash/DND Flash
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